Starting MAKE...
creating project.mk 
lib/csd.asm
lib/csdhl.asm
lib/csdint.asm
lib/csdtable.asm
lib/ezi2cs.asm
lib/ezi2csint.asm
lib/psocconfig.asm
lib/psocconfigtbl.asm
./boot.asm
./main.c
Linking..
LMM info: area 'InterruptRAM' uses 87 bytes in SRAM bank 0
LMM info: area 'ram2' item of 68 bytes allocated in SRAM page 0
LMM info: area 'ram1' item of 60 bytes allocated in SRAM page 0
LMM info: area 'bss' item of 30 bytes allocated in SRAM page 0
LMM info: area 'data' item of 2 bytes allocated in SRAM page 0
LMM info: area 'data' item of 23 bytes allocated in SRAM page 1
LMM info: area 'virtual_registers' uses 4 bytes in SRAM page 1
idata dump at output/Krypton_CSD_part_test.idata
  ROM 11% full. 3595 out of 32768 bytes used (does not include absolute areas).
  RAM 16% full. 274 bytes used (does not include stack usage).
Built with ICCM8C STD V7.05.00
 
Krypton_CSD_part_test - 0 error(s) 0 warning(s) 15:11:51

