;Send line to scan CapSEnce Buttons (P0[5], P0[6])
;To make this example works you should connect 
;relative pins (I2CClock - P12[0], I2CData - P12[1])

;1.Scan CapSense Buttons (PSoC5)
r 04 @1key1 @0key1 @1key2 @0key2
