;
; Texas Instruments CCxxxx USB Serial Port Setup File
;
; Based on Windows USB CDC ACM Setup File
; Copyright (c) 2000 Microsoft Corporation
; Copyright (c) 2013 Texas Instruments Inc

[Version]
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%PROVIDER%
DriverVer=04/05/2013,1.2.0.0
CatalogFile=ccxxxx_usb_cdc.cat

[Manufacturer]
%MFGNAME%=DeviceList,NTx86,NTamd64


[DeviceList.NTx86]
%DESC_SRFEB%    = DriverInstall, USB\VID_0451&PID_16B6
%DESC_CC2511%   = DriverInstall, USB\VID_0451&PID_16A4
%DESC_CC1111%   = DriverInstall, USB\VID_0451&PID_16A6
%DESC_CC2531%   = DriverInstall, USB\VID_0451&PID_16A8
%DESC_CC2540%   = DriverInstall, USB\VID_0451&PID_16AA
%DESC_CC2544%   = DriverInstall, USB\VID_0451&PID_16C5
%DESC_CC2538%   = DriverInstall, USB\VID_0451&PID_16C8
%DESC_CCXXXXBL% = DriverInstall, USB\VID_0451&PID_16C7
%DESC_REMOTINP% = DriverInstall, USB\VID_0451&PID_16B1

[DeviceList.NTamd64]
%DESC_SRFEB%    = DriverInstall, USB\VID_0451&PID_16B6
%DESC_CC2511%   = DriverInstall, USB\VID_0451&PID_16A4
%DESC_CC1111%   = DriverInstall, USB\VID_0451&PID_16A6
%DESC_CC2531%   = DriverInstall, USB\VID_0451&PID_16A8
%DESC_CC2540%   = DriverInstall, USB\VID_0451&PID_16AA
%DESC_CC2544%   = DriverInstall, USB\VID_0451&PID_16C5
%DESC_CC2538%   = DriverInstall, USB\VID_0451&PID_16C8
%DESC_CCXXXXBL% = DriverInstall, USB\VID_0451&PID_16C7
%DESC_REMOTINP% = DriverInstall, USB\VID_0451&PID_16B1


;------------------------------------------------------------------------------
;  Windows 32-bit sections
;------------------------------------------------------------------------------

[DriverInstall.NTx86]
include=mdmcpq.inf
CopyFiles=FakeModemCopyFileSection
AddReg=DriverRegistryKeys

[DriverInstall.NTx86.Services]
AddService=usbser, 0x00000002, DriverService


;------------------------------------------------------------------------------
;  Windows 64-bit sections
;------------------------------------------------------------------------------

[DriverInstall.NTamd64]
include=mdmcpq.inf
CopyFiles=FakeModemCopyFileSection
AddReg=DriverRegistryKeys

[DriverInstall.NTamd64.Services]
AddService=usbser, 0x00000002, DriverService


;------------------------------------------------------------------------------
;
;------------------------------------------------------------------------------

[DriverRegistryKeys]
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverService]
DisplayName   = %SERVICE%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %12%\usbser.sys


;------------------------------------------------------------------------------
;  String Definitions
;------------------------------------------------------------------------------

[Strings]
PROVIDER      = "Texas Instruments"
MFGNAME       = "Texas Instruments"
SERVICE       = "TI USB CDC Driver"
DESC_SRFEB    = "TI SmartRFEB USB CDC Serial Port"
DESC_CC1111   = "TI CC1111 USB CDC Serial Port"
DESC_CC2511   = "TI CC2511 USB CDC Serial Port"
DESC_CC2531   = "TI CC2531 USB CDC Serial Port"
DESC_CC2538   = "TI CC2538 USB CDC Serial Port"
DESC_CC2540   = "TI CC2540 USB CDC Serial Port"
DESC_CC2544   = "TI CC2544 USB CDC Serial Port"
DESC_CCXXXXBL = "TI CCxxxx Generic USB CDC Boot Loader"
DESC_REMOTINP = "RemoTI Network Processor"
